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Rate Sheet
	Nation Rise Unit Rate Sheet
	Unit Rate
	Furnish Materials
	Rate (Equipment)
	Rate (Labor Only)

	Erection:

	WTG component crew unloading $ per hour rate
	
	
	
	

	Base/LM installation per hour 
	
	
	
	

	Blade Roll / Set Hub per hour
	
	
	
	

	Top Out Crew per hour 
	
	
	
	

	Civil:

	Adder to change 8” cement stabilized section with 6% cement with 8” finish on top to 8” cement stabilized section with 7% cement with 8” finish on top.
	
	
	
	

	Adder to change 8” cement stabilized section with 6% cement with 8” finish on top to 8” cement stabilized section with 8% cement with 8” finish on top.
	
	
	
	

	Adder to change 8” cement stabilized section with 6% cement with 8” finish on top to 8” cement stabilized section with 9% cement with 8” finish on top.
	
	
	
	

	Adder to change 8” cement stabilized section with 6% cement with 8” finish on top to 8” cement stabilized section with 10% cement with 8” finish on top.
	
	
	
	

	Scarify & re-compact after cement stabilization per SY
	
	
	
	

	Over Excavations $ / CY
	
	
	
	

	Rock Excavations $ / CY
	
	
	
	

	Select fill for over excavations $ / CY
	
	
	
	

	Hauling unsuitable soils off site $ / CY
	
	
	
	

	Low water crossings  (EA)
	
	
	
	

	$ / CY aggregate - delivered to site
	
	
	
	

	Concrete installation $ / CY (5000)
	
	
	
	

	Rebar Installation $ / lb
	
	
	
	

	Access Road Gate (Provide Spec)
	
	
	
	

	Cattle Guards 
	
	
	
	

	Collection:

	Main Collection Trenching  $ / ft
	
	
	
	

	4/0 AWG – Al cable splice
	
	
	
	

	500 MCM – Al cable splice
	
	
	
	

	1250 MCM – Al cable splice
	
	
	
	

	Trenching for fiber or ground only $ / ft.
	
	
	
	

	Directional Drilling $ / ft 
	
	
	
	

	Importing Select Fill $ / CY
	
	
	
	

	Substation:

	Foundation Install $ / CY
	
	
	
	

	Crush Stone Furnish and Install $ /  CY
	
	
	
	

	HV Tech
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