Logger Files are from AcuEnergy Meter installed at 20CPD in 2021 in connection with the solar PV installation. This meter reads the total building load including BOTH the grid contribution and solar PV contribution. 
The meter can be accessed on the 20CPD maintenance network at port 192.168.2.251 to stop or modify these reports. 

